

(608) 243-0330 Environmental Health

Source Jefferson County Health Dept. Indiana

Source Jefferson County Health Dept 812-273-1942

* Backflow prevention devices required on threaded hose faucets and chemical mixing stations (ASSE 1011, ASSE 1052 or ASSE 1001 at 7’6” above floor finish)
* Air Gaps required for prep sinks, dipper wells, ice machines, ice bins, spray arm hose reels, thermalizers, sanitize compartment of dishwashing sink, dishmachines and any connection between food/beverage equipment and discharge piping.
* Swimming pool water fill lines require air gaps. Backwash water can discharge via air break or air gap.

***Consult and use licensed plumber for compliance***

